[image: ]
[image: ]
image1.png
Technical Specificati

Ordering Information: 700223
Power Supply / Input Voltage Internal Battery or 120240V 50/60 Hz
Supply Power Required 200
Rated Max Voltage 120KV Peak /185 KV RMS @ 0.1 He
Rated Max Current 1 Amp
Operating Frequencies 0.01 10 0.1Hz (Default 0.1Hz)
Filter Capacitance nF
Coupling Capacitance nF
Input Impedance 10kOhm / 50pF
Sampling Rate 125 MHz (Ver2 - 200MHz)
Bandwidth 100 MHz
Measuring Range 12 miles @ 260 /oS
20km @80 mius
VOP Range (V/2) 10m-150 m/uS or 32490f¢/uS
PD Background Level <0pC
PD Location Accuracy %
PD Resolution 0.2m/0.6ft and 0.1pC
Voltages Synchronization Automatic

Manual and Automatic

12°x10"x 31" (300 x 250 x 785mm)
471bs/21.2 kgs

12" x 10" 27" (300 x 250 x 690mm)

441bs /199 kgs
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Environmental:
Storage
Operating

CALIBRATOR (ACC. IEC 60270)
included with every PD60-2 system

Ordering Information:

Output

Size and Weight

DIAGNOSTICS SOFTWARE: HVD SUITE
(included with all PD / PDTD systems)

Features

Windows Compatible *

* Note these sre not ncluded in zcope of upply:

4F° 10 150F° /-20C" 10 65C
23F 10 113/ 5C 10 45C°

700222
100pC 0 10nC

0716.@24"x65"x13"
0.3 kg @ 60mm x 164mm x 33mm

Automatic and Manual Control of HVA and PD Test System Fully Guided Measurement
Process Storage Database PD Display - Raw Data, Calibration Pulses, PD Amplitude versus
Distance, PD Amplitude versus Phase, PD Location (PD mapping), PDIV and PDEV,
Automatic Distance to PD fault location, Noise and filtering options.

Windows 7, 8,10 64 bit Operating Systems

- Laptop/PC s required to operate PD & PDTD - systems include Laptop/PC with order, uless otherwise specified.

- An HUA Series VLF AC s required t operate with his instrument and i not automaticaly included.




